;
; VAG-COM label file
;
; VW Phaeton (3D)
;
; Component: Tire Pressure Monitoring -J502- (#65)
;
; p/n: 3D0 907 273 A
;      3D0 907 273 B
;      3D0 907 273 C
;      3D0 907 273 D
;      3D0 907 273 E
;
; includes measuring blocks
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modified: 11/05/2004
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; Measuaring block informations
;
;---------------------------------------------------
;
;
001,0,Front Left Wheel
001,1,Wheel position
001,2,Wheel,temperature,Specified value: -40...120 °C
001,3,Relative actual,pressure,Specified value: 0...5.37 bar
001,4,Relative spec.,pressure,Specified value: 0...5.37 bar
;
002,0,Front Left Wheel
002,2,Remaining,battery life,Specified value: 0...99 month
;
004,0,Front Right Wheel
004,1,Wheel position
004,2,Wheel,temperature,Specified value: -40...120 °C
004,3,Relative actual,pressure,Specified value: 0...5.37 bar
004,4,Relative spec.,pressure,Specified value: 0...5.37 bar
;
005,0,Front Right Wheel
005,2,Remaining,battery life,Specified value: 0...99 month
;
007,0,Rear Left Wheel
007,1,Wheel position
007,2,Wheel,temperature,Specified value: -40...120 °C
007,3,Relative actual,pressure,Specified value: 0...5.37 bar
007,4,Relative spec.,pressure,Specified value: 0...5.37 bar
;
008,0,Rear Left Wheel
008,2,Remaining,battery life,Specified value: 0...99 month
;
010,0,Rear Right Wheel
010,1,Wheel position
010,2,Wheel,temperature,Specified value: -40...120 °C
010,3,Relative actual,pressure,Specified value: 0...5.37 bar
010,4,Relative spec.,pressure,Specified value: 0...5.37 bar
;
011,0,Rear Right Wheel
011,2,Remaining,battery life,Specified value: 0...99 month
;
013,0,Spare Wheel
013,1,Wheel position
013,2,Wheel,temperature,Specified value: -40...120 °C
013,3,Relative actual,pressure,Specified value: 0...5.37 bar
013,4,Relative spec.,pressure,Specified value: 0...5.37 bar
;
014,0,Spare Wheel
014,2,Remaining,battery life,Specified value: 0...99 month
;
015,4,Battery voltage,Specified value: Ub. i.O./Ub. n.i.O./no Signal
;
017,2,Voltage supply,,Specified value: 0...25.5 V
017,3,Vehicle status,,Specified value: 1 = stand/0 = driving
017,4,Tachometer,signal,Specified value: 0...255 km/h
;
018,1,Outside,temperature,Specified value: -40...120 °C
;
021,1,Antenna,diagnosis,inactive/wait/Message End
;
