;
; VAG-COM label file
;
; VW Phaeton (3D)
;
; Component: Level Control System -J197- (#34)
;
; p/n: 3D0 907 553 A
;      3D0 907 553 B
;      3D0 907 553 C
;
; includes measuring blocks
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modified: 11/05/2004
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; Measuaring block informations
;
;---------------------------------------------------
;
;
001,1,Voltage,Terminal 15,Specified value: 0...20 V
001,2,Voltage,Terminal 30,Specified value: 0...20 V
001,3,Vehicle speed,,Specified value: 0...250 km/h
001,4,Starter,Terminal 50,Specified value: Term. 50 off/Term. 50 on
;
002,1,Door,identification,Door open/Door closed
002,2,Rear lid,,Specified value: Lid open/Lid closed
002,3,Right Sensor,Supply Voltage,Specified value: 0...10 V
002,4,Left Sensor,Supply Voltage,Specified value: 0...10 V
;
003,3,Level switch,,Specified value: active/inactive
003,4,Compressor,relay,Specified value: Relay off/Relay on,
;
004,0,Deviation from normal level
004,1,Front Left,,Specified value: -127...+128 mm
004,2,Front Right,,Specified value: -127...+128 mm
004,3,Rear Left,,Specified value: -127...+128 mm
004,4,Rear Right,,Specified value: -127...+128 mm
;
005,0,Absolute vehicle height
005,1,Front Left,,Specified value: 0...255
005,2,Front Right,,Specified value: 0...255
005,3,Rear Left,,Specified value: 0...255
005,4,Right Rear,,Specified value: 0...255
;
006,1,Compressor,temperature,Specified value: -40...+140 °C
006,2,Pressure signal,,Specified value: 0...20 bar
006,3,Relief valve,,Specified value: on/off
006,4,Pressure,reservoir valve,Specified value: on/off
;
007,0,Differential lock valve switch condition
007,1,Front Left,,Specified value: off/on
007,2,Front Right,,Specified value: off/on
007,3,Rear Left,,Specified value: off/on
007,4,Rear Right,,Specified value: off/on
;
009,0,Average height deviation
009,3,Front Axle,,Specified value: -127...+128 mm
009,4,Rear Axle,,Specified value: -127...+128 mm
;
010,0,Vehicle level deviation
010,1,Left Front,,Specified value: -127...+128 mm
010,2,Right Front,,Specified value: -127...+128 mm
010,3,Left Rear,,Specified value: -127...+128 mm
010,4,Right Rear,,Specified value: -127...+128 mm
;
011,0,Shock absorber valve current
011,1,Left Front,,Specified value: 0...2050 mA
011,2,Right Front,,Specified value: 0...2050 mA
011,3,Left Rear,,Specified value: 0...2050 mA
011,4,Right Rear,,Specified value: 0...2050 mA
;
012,0,Body acceleration signal
012,1,Left Front,,Specified value: 0...5 V
012,2,Right Front,,Specified value: 0 .. 5 V
012,3,Rear Axle,,Specified value: 0 .. 5 V
;
013,0,Wheel acceleration signal
013,1,Left Front,,Specified value: 0...5 V
013,2,Right Front,,Specified value: 0...5 V
013,3,Left Rear,,Specified value: 0...5 V
013,4,Right Rear,,Specified value: 0...5 V
;
14,1,Condition CDC-button,unbetätigt/betätigt,
14,2,current shock absorber detection,0/1/2/3,komfort/normal/sport 1/sport 2
14,3,CDC display,ein/aus,
;
015,1,Steering angle,,Specified value: +/- 720 °
015,2,Vehicle speed,,Specified value: 0...250 km/hs
;
