;
; VAG-COM label file
;
; VW Phaeton (3D)
;
; component: Central Electronics -J519-  (#09)
;
; p/n: 3D0 937 049 E
;      3D0 937 049 G
;      3D0 937 049 H
;
; includes measuring blocks
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modified: 11/05/2004
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; Measuaring block informations
;
;---------------------------------------------------
;
;
001,1,Parking light,switch,Specified value: off/on
001,2,Low beam,headlight switch,Specified value: off/on
001,3,Light switch for,automatic light,Specified value: off/on
001,4,Light switch for,emergency flasher,Specified value: active/inactive
;
002,0,Light switches
002,1,Rear fog light,,Specified value: off/on/not installed
002,2,Fog light,,Specified value: off/on/not installed
002,3,Back-up light,,Specified value: off/on
002,4,[N/A]
;
003,0,Dimming stage
003,1,Increase,button,Specified value: active/inactive
003,2,Decrease,button,Specified value: active/inactive
;
004,3,Engine hood,switch,Specified value: off/on
;
005,0,Mirror adjustment switch
005,1,Y-Axis,(minus),Specified value: active/inactive
005,2,Y-Axis,(plus),Specified value: active/inactive
005,3,X-Axis,(minus),Specified value: active/inactive
005,4,X-Axis,(plus),Specified value: active/inactive
;
006,0,Mirror system
006,1,Left mirror,selection,Specified value: active/inactive
006,2,Right mirror,selection,Specified value: active/inactive
006,3,Folding in,mirror,Specified value: active/inactive
006,4,Heated mirror,switch,Specified value: off/on
;
007,0,Voltage
007,1,Terminal 15,,Specified value: Term. 15 on/Term. 15 off
007,2,Terminal X,,Specified value: Term. X on/Term. X off
007,3,System,battery,Specified value: 6...15 V
007,4,Starter,battery,Specified value: 6...15 V
;
008,1,Left low,beam headlight,Specified value: off/on
008,2,Right low,beam headlight,Specified value: off/on
008,3,Left high beam,,Specified value: off/on
008,4,Right high beam,,Specified value: off/on
;
009,0,Position lights
009,1,Left,position light,Specified value: off/on
009,2,Right,position light,Specified value: off/on
;
010,1,Turn signal,light left,Specified value: off/on
010,2,Turn signal,light right,Specified value: off/on
010,3,Fog light,left/right,Specified value: off/on
;
011,1,Left turn,signal lever,Specified value: off/on
011,2,Right turn,signal lever,Specified value: off/on
011,3,Left parking,light switch,Specified value: off/on
011,4,Right parking,light switch,Specified value: off/on
;
012,1,Headlamp,flasher switch,Specified value: off/on
012,2,High beam switch,,Specified value: off/on
012,3,Switch for horn,,Specified value: off/on
012,4,Front washing,switch,Specified value: off/on
;
013,1,Load management,intervantion,Specified value: active/inactive
013,2,max. reached,shut-off priority,Specified value: 0...254
;
014,0,Heated mirrors
014,1,Driver door,heated mirror,Specified value: off/on
014,2,Passenger door,heated mirror,Specified value: off/on
;
015,0,Rotary traps
015,1,Driver door,rotary trap,Specified value: open/closed
015,2,Passenger door,rotary trap,Specified value: open/closed
015,3,Rotary trap,LR door,Specified value: open/closed
015,4,Rotary trap,RR door,Specified value: open/closed
;
016,1,Footwell light,dimming stage,Specified value: 0...100 %
016,2,Terminal DFM,,Specified value: 0...255 %
016,3,Outside,temperature,Specified value: 0...255 °
016,4,Selector,lever info,Specified value: 0...15
;
