;
; VAG-COM Measuring Block Labels for
; Klima Controller p/n 4A0-820-043-xx
; From 1996 European Audi A6
;
; Contributed by Ole Gudmund Bjørk
;
1,0,Compressor
1,1,Switch-off status,0=OK
1,2,Voltage AC Clutch
1,3,Voltage at,Terminal 75
1,4,Not in use
;
2,0,Temperature Regulator Flap
2,1,Actual value,sensor G92
2,2,Specified value,sensor G92
2,3,Learned value,Heat(5-30)
2,4,Learned value,Cool(200-250)
;
3,0,Center Air Flap
3,1,Actual value,sensor G112
3,2,Specified value,sensor G112
3,3,Learned value,Foot/Defr.(5-30)
3,4,Learned value,Instrum.(200-250)
;
4,0,Footwell/Defroster flap
4,1,Actual value,sensor G114
4,2,Specified value,sensor G114
4,3,Learned value,Defroster(5-30)
4,4,Learned value,Footwell(200-250)
;
5,0,Air Flow Flap
5,1,Actual value,sensor G113
5,2,Specified value,sensor G113
5,3,Learned value,Recycle on
5,4,Learned value,Recycle off
;
6,0,Outside air temperature
6,1,Air temp lower,of G89 and G17
6,2,Temp fresh air,duct G89
6,3,Air temp LF,bumper G17
6,4,Temp fresh,airblower G109, 
;
7,0,Interior temperature
7,1,Temp. upper,sensor G86
7,2,Temp. lower,sensor G56
7,3,Calculated temp.
7,4,Engine coolant,temp G110
;
8,0,Fresh Air Blower and Lights
8,1,Specified volt.,air blower V2
8,2,Actual,volt.,air blower V2
8,3,Voltage Terminal,58D
8,4,Parklights,0=OFF 1=ON
;
9,0,Engine. Compressor and vehicle speed.
9,1,Engine speed,1.28
9,2,Compr. speed,1
9,3,0=No vehiclesp.,detected
9,4,0=Voltage,E87D < 2V
;
10,0,Kick-down, Coolant temp.
10,1,Kickdown sw.,0=OFF 1=ON
10,2,Temp sw. F76,0=OFF 1=ON
10,3,Compr. output,0=OFF 1=ON
10,4,Highpr. sw F118,0=OFF 1=ON


