;
; VAG-COM Measuring Block Labels for
; All OBD-I VR6, ECU p/n 021-906-258-xx
;
; Posted by Uwe Ross 3/10/2001
; Modified by Chris Gaskell 15/3/2001  England - UK
;             (Ref.Bentley - Corrado/VAG 1551 UK Print Out)
; Now VERIFIED 18/3/2001
;
1,0,General Engine Data
1,1,RPM,Engine Speed
1,2,Coolant,Temperature
1,3,O2,Active
1,4,Ignition,Timing
;
2,0,General Engine Data
2,1,RPM,Eng Speed
2,2,Injector,ON Time
2,3,Battery,Voltage
2,4,EGR Temp,(if available)
;
3,0,General Engine Data
3,1,RPM,Engine Speed
3,2,Engine,Load (%)
3,3,Throttle Angle,<°
3,4,Intake Air,Temp - Manifold
;
4,0,General Engine Data
4,1,RPM,Engine Speed
4,2,Engine,Load (%)
4,3,Vehicle,Speed
4,4,Switch Postn,Binary Codes
;
; Binary Codes - Grp 04, Measuring Channel 4.
;   10000 - Acceleration enrichment
;   01000 - Wide Open Throttle
;   00100 - Partially Open Throttle
;   00010 - Idle Position
;   00001 - Deceleration
;   00000 - Switch position NOT OK
;           (activate DTC memory again if this code appears)
;
5,0,Idle Control
5,1,RPM,Engine Speed
5,2,ISV,Adaptation
5,3,ISV,Duty Cycle(%)
5,4,Switch Postn,Binary Codes
;
; Binary Codes - Grp 05, Measuring Channel 4.
;   10-00 - A/C Compressor ON
;   01-00 - A/C Compressor OFF
;   00-10 - Transmission engagement (for automatic transmission ONLY)
;   00-01 - Drive Step (for automatic transmission ONLY)
;
6,0,Fuel Trim (O2 Sensor)
6,1,O2,Active
6,2,Idle,Adapted Value
6,3,Part Throttle,Adapted Value
6,4,Full Throttle,Adapted Value
;
;  Less than 1.0 is rich, greater than 1.0 is lean
;