;
; VAG-COM Measuring Block Labels file.
; Module 17 -- Instrument cluster Long Life
; 
; from  2000 Audi A6
;
; p/n  :  4B0-920-830
; 
; Login 13861 for for change of run  
; channel 9 :Run is less than 100 kms
;
; **Modification history**
; created:  Dima Suhov, 20 July 2002.
; please email any comments or corrections: terma@svitonline.com
;
; **********************************************************************
1,1,Car speed,km/h
1,2,Engine speed,rpm
1,3,Oil presure switch,2<min
1,4,time
;
2,1,Mileage/km counter,(km)
2,2,Fuel gaugel,0...100 l
2,3,Gauge stock fuel,70...270 Ohm
2,4,Ambient temperature,-40...+70 °C
;
3,1,Coolant temperature,°C
3,2,-
3,3,-
3,4,-
;
4,0,Next blok 10
;
5,0,Next blok 10
;
6,0,Next blok 10
;
7,0,Next blok 10
;
8,0,Next blok 10
;
9,0,Next blok 10
;
10,0,Change run,Login 13861
10,1,channel 30,120...136
10,2,Adapting fuel sender,128=0
10,3,channel 9,00001=10km
10,4,Mileage/km counter,(km)
;
11,1,channel 4,1...6
11,2,Language,1=DE 2=EN
11,3,channel 3,85...115
11,4,charge fuel,100=100%
;
12,0,Since servis
12,1,channel 40
12,2,8=800km
12,3,channel 41
12,4,10=10days
;
13,0,Oil servis,min...max
13,1,channel 42
13,2,min run,15=15000km
13,3,channel 43
13,4,max run,30=30000km
;
14,0,max time to insr.
14,1,channel 44
14,2,1=1day,max 730
14,3,---
14,4,---
;
15,1,channel 45
15,2,Quality oil,1...4
15,3,channel 46
15,4,Quantity fuel,l
;
16,1,channel 47
16,2,Parameter of soot
16,3,channel 48
16,4,Thermal loading
;
17,0,Next blok 22
;
18,0,Next blok 22
;
19,0,Next blok 22
;
22,0,Immobilizer,1=yes 0=no
22,1,Engine start enabled,1=yes 0=no
22,2,Response engine,1=yes 0=no
22,3,Key OK,1=yes 0=no
22,4,No. of keys,max 8
;
23,0,Immobilizer
23,1,Autor variable code,1=yes 0=no
23,2,Key blocked,1=yes 0=no
23,3,Autor fixed code,1=yes 0=no
23,4,Immobilizer status,6=OK
;
24,0,Immob.bloc.time
24,1,Instrum. block.,min
24,2,channel 50 block.,min
24,3,PIN block.,min
24,4,Key block.,min

;
25,0,Immobilizer
25,1,CAN-com.
25,2,---
25,3,---
25,4,---
;
26,0,Next blok 50
;
27,0,Next blok 50
;
28,0,Next blok 50
;
50,1,Mileage/km counter,(km)
50,2,Engine speed,rpm
50,3,Oil temperature,°C
50,4,Coolant temperature,°C
;
51,0,Next blok 125
;
52,0,Next blok 125
;
53,0,Next blok 125
;
125,0, CAN-Drive,
125,1,Motor,1=OK
125,2,Gear,1=OK
125,3,ABS,1=OK
125,4,ADR,1=OK
;
126,0, CAN-Drive
126,1,Klima,1=OK
126,2---
126,3---
126,4---
;
127,0,Next blok 130
;
128,0,Next blok 130
;
129,0,Next blok 130
;
130,0, CAN-Comfort
130,1,Pres.in trunks,1=OK
130,2,Indep.heater,1=OK
130,3,---
130,4,Parking,1=OK
;
131,0,Next blok 140
;
132,0,Next blok 140
;
133,0,Next blok 140
;
140,0, CAN-Inform.
140,1,Radio,1=OK
140,2,Telefon,1=OK
140,3,Navig,1=OK
140,4,Telematik,1=OK
;
141,0,END
;
142,0,END
;
143,0,END
;
;
;<end of file>