; VAG-COM Measuring Block Labels 
; VW Transporter T4 1991-->
; Code: ACV,AHY,AJT
; ECU:  074-906-018
;
;0,0,Measured Value Block
;0,1,Engine speed
;0,2,Commencement, of injection
;0,3,Accelerator, pedal position
;0,4,Quantify, injected
;0,5,Charge, presure
;0,6,Ambient, presure
;0,7,Coolant, temperature
;0,8,Intake manifold, temperature
;0,9,Fuel,temperature
;0,10,Mass of air, drawn in
;
1,0,Quantify, injected
1,1,Engine speed
1,2,Qty injected, mg/h
1,3,Vol. from, slide valve
1,4,Coolant, temperature              
;
2,0,Idling speed
2,1,Engine speed
2,2,Accel. pedal, position
2,3,Operating, condition
;101 A/C comp on
;010 Idling speed switch closed (accel. pedal position below 17%)
2,4,Coolant, temperature
;
3,0,Exhaust gas, recirculation
3,1,Engine speed,
3,2,Mass air, drawn spec
3,3,Mass air, drawn actual
3,4,EGR,duty cycle
;
4,0,Commencement, of injection
4,1,Engine speed,
4,2,Comm. of inject., specified
4,3,Comm. of inject., actual
4,4,Comm. inject valve, duty cycle
;
5,0,Start conditions
5,1,Engine speed,
5,2,Start quantify,
5,3,Comm. of inject., actual
5,4,Coolant, temperature
;
6,0,Switch positions
6,1,Speed
6,2,Brake pedal, monitor
;011 Brake pedal operated (brake light switch)
;011 Brake pedal operated (brake pedal switch)
;100 Clutch pedal operated (Clutch pedal swich open)
6,3,CCS
;000000 Cruise control switch to OFF
;000001 Cruise control switch to ON
;000101 SET button
:001001 Speed resume Switch to RES
;010001 Brake pedal operated (brake pedal switch)
;100001 Clutch pedal operated (Clutch pedal swich open)
6,4,CCS,
;0 Vehicles with cruise control system switched off
;1 Vehicles with cruise control system switched on
;255 Vehicles without cruise control system or  cruise control system not activated
;
7,0,Temperatures
7,1,Fuel temp.
7,2,No display
7,3,Intake manifold, temp. 
7,4,Coolant, temperature
;
8,0,Injected quantify, limitation
8,1,Engine speed,
8,2,Quantify injected, driver's req.
8,3,Injected Qty limit.,torque map
8,4,Injected Qty limit.,opacity map
;
9,0,Injected Qty limitation 2
9,1,Engine speed
9,2, quantify injected, CSS active
9,3,Injected Qty limit.,AT trq limit.
9,4,Voltage supp.,piston movem. sdr
;
10,0,Air quantities,
10,1,Mass air, drawn actual
10,2,Ambient, presure
10,3,Charge, presure
10,4,Accel. pedal, position
;
11,0,Charge presure, control
11,1,Engine speed
11,2,Charge presure,specified
11,3,Charge presure,actual
11,4,Charge pres ctrl valve,duty cycle
;
12,0,Glow plug, system
12,1,Not relevant
12,2,Glow period
12,3,V supply, from ctrl unit
12,4,Coolant, temperature
;
13,0,Idling speed smooth running control (ACV,AHY)
13,1,Qty inject. dev., cyl. 1-3
13,2,Qty inject. dev., cyl. 2-3
13,3,Qty inject. dev., cyl. 4-3
13,4,Qty inject. dev., cyl. 5-3
; Engine code AJT
; 13,1, Cyl 1 quantify injected deviantion from mean quantify injected
; 13,2, Cyl 2 quantify injected deviantion from mean quantify injected
; 13,3, Cyl 3 quantify injected deviantion from mean quantify injected
; 13,4, Cyl 4 quantify injected deviantion from mean quantify injected
;
14,0,Idling speed smooth running control (only AJT)
;14,1,Cyl 5 quantify injected deviantion from mean quantify injected
14,2, No display
14,3, No display
14,4, No display
;
18,0,Switch, positions
18,1,Speed,km/h
18,2, CSS status
; Vehicle with speedometer 0X
; Vehicle with tachograph 1X
;
19,0,Qty setting, mechannism
19,1,V modul. pist. movem., sender stop limit
19,2,V modul. pist. movem., sender start limit
19,3,No display
19,4,No display
;
;EOF
;
;
