;
; VAG-COM Measuring Block Labels file.
; Golf IV Climatronic (A/C) 3B1 907 044B
;
; contributed by Jens Ulmer, 27.08.2001
;
1,0,General values
1,1,A/C clutch,sw-off cond. 1-12 
1,2,Eng. speed recog,(0=no/1=yes)
1,3,Road Speed
1,4,Standing time,(0-240 min.)
;
2,0,Temperature Regulator Flap
2,1,Measured value
2,2,Specified value
2,3,Position: air,supply cooled
2,4,Position: air,supply heated
;
3,0,Center Air Flap
3,1,Measured value
3,2,Specified value
3,3,Position: air,flow to panel
3,4,Position: air,flow to footwell
;
4,0,Footwell/Defroster Flap
4,1,Measured value
4,2,Specified value
4,3,Position: air,flow to footwell
4,4,Position: air,flow to defroster
;
5,0,Air Flow Flap
5,1,Measured value
5,2,Specified value
5,3,Position:,fresh air
5,4,Position:,recirculating
;
6,0,Temperatures & Photo Sensor
6,1,Temp. displayed,on panel
6,2,Temp. air,intake duct
6,3,Outside air,temperature
6,4,Sun photo,sensor (0-120%)
; 
7,0,More temperatures
7,1,Outlet temp.,panel (G191)
7,2,Outlet temp.,floor (G192)
7,3,Panel temp.,near LCD (G56)
7,4,n/a
;
8,0,Voltages
8,1,Specif. Voltage,air blower
8,2,Measured Voltage,air blower
8,3,Measured Voltage,Terminal 15
8,3,Measured Voltage,A/C clutch
;
