;
; VAG-COM Measuring Block Labels file.
; S8 Xenon Head Lights Range Adjusting Controller
; Filename:4B0-907-357-C.LBL
;
;   Controller: 4B0 907 357 C 
;       Module: 55
;    Component: dynamische LWR D05 
;       Coding: 00001
;
; **Modification History**
; Created:  Dave Eaton, 3rd February 2004
; Modified: Dave Eaton, 5th February: Test & Corrections
; Corrections to: Dave.Eaton@clear.net.nz
;
;
; **********************************************************************
1,0,Voltages and Speed
1,1,Power Supply,0 - 15V
1,2,Switch State,0=Off 1=On
1,3,Speed,Km/h
1,4,Acceleration,0 - 7m/s/s
;
2,0,Axles Sensors and Adaptation
2,1,Front Level sensor,G78 (1.56-3.45V)
2,2,Rear Level sensor,G76 (0.5-4.5V)
2,3,Actuator Motors,Travel % from 0
2,4,Time Constant,(to 63% adj.)
;
;End of File
