;
; Note from Ross-Tech:
; Many of the texts in this file are WAY too long.
; Remove -XXX from file name to test, but expect
; problems until texts are shortened.
;

; Created by Kim Andersen:gasarm@post.tele.dk
; Engine code: AEH-AKL Golf 1998>,Bora 1999>
; ECU Number : 06A-906-019 
; Engine type: 1.6 I R4/2V SIMOS HS 2272
; Coding:04000
; Documentation used:"Erwin WorkShop Manual Golf 1998>,Bora 1999>
;                     Simos injection and ignition system"


;0,0 Measured value blocks(Engine running at idle speed	)			
;0,1 Intake air temperature						;84-158		;15-71°Celius
;0,2 Engine control unit supply voltage					;98-147		;10-15 Volt
;0,3 Coolant temperature 						;170-211	;80-110°Celius
;0,4 Air mass drawn in							;14-30		;76-164 mg/lift
;0,5 Lambda probe voltage						;0-50		;0.0-1.0 Volt
;0,6 Lambda learnt value at idling					;0-100		;-0.8-0.8 ms
;0,7 Operation condition of Lanbda control				;See measured value block 99
;0,8 Throttle valve angle						;4-12		;1.9-5.7<°Degree 
;0,9 Injection period							;2-4		;2-4.1 ms
;0.10 Engine speed (idling speed)					;23-27		;760-880 RPM

1,0,Basic functions
1,1,Engine speed,760-880 rpm 
1,2,Coolant temperature,80-110°Celius
1,3,Lambda probe voltage,0.00-1.00 Volt
1,4,Adj.condi.matching throttle valve,00000010
;xxxxxxxx
;1        Fault identified by self-diagnosis
; 1       Signal from automatic gearbox
;  1      Air conditioner switched on
;   1     Idling speed switch open
;    1    Fault in Lambda control
;     1   Throttle valve open (angle check)
;      1  Engine running
;       1 Coolant temperature less than 80 °Celius
;


2,0,Basic Functions 
2,1,Engine speed,760-880 rpm
2,2,Airflow (engine load),76-164 mg/H
2,3,Road speed,0 km/h
2,4,Engine operating,0100

3,0,Basic functions
3,1,Engine speed,760-880 rpm
3,2,Airflow (engine load),76-164 mg/H
3,3,Throttle valve angle, 1.9-5.7<°Degree
3,4,Throt.valve posi.duty cycle, -100-100 %

4,0,Basic functions
4,1,Engine speed, 760-880 rpm 
4,2,Airflow (engine load), 76-164 mg/H
4,3,Injection period, 2.0-4.10 ms
4,4,Air mass drawn in, 1.8 - 3.2 g/s

5,0,Basic functions
5,1,Engine Speed (760-880 rpm)
5,2,ECU voltage supply, 10-15 Volt
5,3,Coolant temperature, 80-110°Celius
5,4,Intake air temperature, 15-71°Celius

6,0,Altitude adaption
6,1,Engine speed, 760-880 rpm
6,2,Airflow (engine load), 76-164 mg/H
6,3,Throttle valve angle, 1.9-5.7 <°Degree 
6,4,Altitude correction factor,0.9-1.1

7,0,Idling adjustment
7,1,Throttle valve angle,1.9-5.7<°Degree
7,2,Idling learnt value,0.95-1.05
7,3,Idling learnt value,0.95-1.05
7,4,Engine operating,0100
;xxxx
;1    Overrun
; 1   Idling
;  1  Part throttle
;   1 Full throttle
;


8,0,Idling stabilitation
8,1,Engine speed,760-880 rpm  
8,2,Engine speed (specifi),800-840 rpm
8,3,Idling control,-10-15 %
8,4,Amount of air drawn in,1.0-3.2 g/s

9,0,Idling air requirements
9,1,Idling control,-10-15 %
9,2,Throttle valve status,see label file
9,3,Coolant temperature,80-110°Celius
9,4,Engine speed,760-880 rpm
;xxxxxxxx
;0        Not allocated 
; 0       Not allocated
;  0      Not allocated
;   0     Not allocated
;    1    Fault has occurred during adaption
;     1   No current supply to throttle valve
;      1  Battery voltage too low (below 8V)
;       1 Idling switch open
;


10,0,Lambda control and activated charcoal filter system
10,1,Lambda regulator,-25-25 % 
10,2,Lambda probe voltage,0.00-1.00 Volt
10,3,Activated charcoal valve 1 Duty Cycle,0-20 %
10,4,Lambda correction tank venting is active,-20-2 %


11,0,Lambda learning values
11,1,Injection period,2.00-4.10 ms
11,2,Lambda learnt value idling,-0.1-1.0 ms
11,3,Lambda learnt value part load,0.9-1.15 ms
11,4,Cond.tank breather valve,see label file
;xxxxxxxx
;0        Vacant
; 1       Transition to vapour content check via fuel tank breather valve
;  1      Transition to fuel tank breather valve minimum operating level
;   1     Transition to fuel tank breather valve closure
;    1    Vapour content check via fuel tank breather valve
;     1   Fuel tank breather valve operating normally
;      1  Fuel tank breather valve minimum operating level
;       1 Fuel tank breather valve closed
;


12,0,Lambda control
12,1,Engine speed,760-880 rpm
12,2,Airflow (engine load),76-164 mg/H
12,3,Lambda regulation,-25-25 %
12,4,Lambda probe volt.,0.00-1.00 volt

13,0,Fuel consumption
13,1,Engine speed,760-880 rpm
13,2,Airflow (engine load),76-164 mg/H
13,3,Road speed,0 km/h
13,4,Fuel consumption,0.50-2.00 l/h

14,0,Knock control
14,1,Cyl1 ign.angle retard,0.0°CA 
14,2,Cyl2 ign.angle retard,0.0°CA 
14,3,Cyl3 ign.angle retard,0.0°CA 
14,4,Cyl4 ign.angle retard,0.0°CA 

15,0,Knock control
15,1,Engine speed,760-880 rpm
15,2,Airflow (engine load),76-164 mg/H
15,3,Cyl1 ign.angle retard,0.0°CA 
15,4,Cyl2 ign.angle retard,0.0°CA 

16,0,Knock control
16,1,Engine speed,760-880 rpm
16,2,Airflow (engine load),76-164 mg/H
16,3,Cyl3 ign.angle retard,0.0°CA 
16,4,Cyl4 ign.angle retard,0.0°CA 

17,0,Knock control
17,1,Volt.Cyl1.knock sensor,0.400-1.300 Vpt
17,2,Volt.Cyl2.knock sensor,0.400-1.300 Vpt
17,3,Volt.Cyl3.knock sensor,0.400-1.300 Vpt
17,4,Volt.Cyl4.knock sensor,0.400-1.300 Vpt


18,0,Torque reduction for automatic gearbox
18,1,Engine speed,760-880 rpm
18,2,Airflow (engine load),74-164 mg/H
18,3,Ign.timing retard gearbox cutin,0.0°CA
18,4,Ignition timing,-6-14°BTDC

19,0,Operation condition
19,1,Engine speed,760-880 rpm
19,2,Selector lever pos.(0 or 1),0
19,3,Air conditioner (0 or 1),0 
19,4,Operation condition,see label file
;xxxxxxxx
;0        Not allocated
; 0       Not allocated
;  0      Not allocated
;   0     Not allocated
;    0    Not allocated
;     1   Clutch pedal switch operated
;      1  Power steering pressure switch F88 activated
;       1 A/C compressor switched on
;


20,0,Lambda control operating condition
20,1,Engine speed,760-880 rpm
20,2,Airflow (engine load),76-164 mg/H
20,3,Coolant temperature,80-110°C
20,4,Lambda operating condi.,see label file
;xxxxxxxx
;1        Fault recorded in memory
; 0       Not allocated 
;  0      Not allocated
;   1     Restricted operation mode
;    1    Lambda control at limit
;     1   Lambda control switched on
;      1  Lambda probe functioning  
;       1 Mixture status: 1= Rich mixture 0= Lean mixture
;


21,0,Throttle valve control adaption 
21,1,Throt.valve control adaption,see label file
21,2,Throt.valve min.position,70-100 %
21,3,Throt.valve emerg.run.posi.,67-100 %
21,4,Throt.valve max.position,0-20 %
;xxxxxxxx
;0        Not allocated			
; 0       Not allocated
;  0      Not allocated
;   0     Not allocated
;    1    Fault has occured during adaption
;     1   No current supply(duty cycle=0)
;      1  Battery voltage too low (below 8V)
;       1 Idling switch open
;


22,0,Position of camshaft in relation to crankshaft
22,1,Engine speed,760-880 rpm
22,2,Airflow (engine load),76-164 mg/H
22,3,No.teeth on Crk.sender(- to +),26-30
22,4,No.teeth on Crk.sender(+ to -),86-90

57,0,Idling speed stabilisation -Air Comp. pressure signal
57,1,Engine speed,760-880 rpm
57,2,Idling speed compres.on/off,800-920 760-880 rpm 
57,3,Air conditioner compres.,ON or OFF
57,4,G65 duty cycle with compr.ON/OFF,10-70 % 1-5 %

66,0,Cruise control system
66,1,Road speed (actual),0 km/h
66,2,Brake clutch and CCS switch position,1000
66,3,Road speed (specified),0 km/h
66,4,Operating cruise control,0000= 0ff 0011= on
;xxxx
;1    Cruise control system available
; 1   Clutch pedal depressed/autom.gearbox always 1
;  1  Brake depressed or for autom.gearbox selector lever in "P" position and ignition switched on (engine stationary)
;   1 Brake depressed or for autom.gearbox selector lever in "P" position and ignition switched on (engine stationary)
;
;xxxx
;1    Resume speed,accelerate (CCS sliding switch at RES)
; 1   save speed/delay (SET button pressed)
;  1  CCS temporarily switched off,memory saved
;   1 CCS switched off
;


98,0,Matching throttle valve control part
98,1,Throt.valve pot.volt,3.70-4.75 Volt
98,2,Throt.valve positioner pot.volt,2.28-4.75 Volt
98,3,Operating of throt.valve,00000000
98,4,Matching of throt.valve control part,00

99,0,Lambda regulation
99,1,Engine speed,760-880 rpm
99,2,Coolant temperature,80-110°C
99,3,Lambda regulation,-25-25 %
99,4,Operating condition of Lambda,0xxx011x

;
















































































































 