;2000 GTi VR6 Engine
;Researched by Bob Taylor
;If you find any problems, please e-mail me the corrections.
;jroberttaylor_20164@yahoo.com
;
;
;
;
;
;
;
;
;
;Block 000 won't display, but I added it here for reference.  (Bentley 01-110)
;
;000,0,Measuring Value Block                     	   Specified Value	            Corresponds To
;000,1,Engine Coolant Temperature					185-205				85-105Deg. C
;000,2,Engine load							-------				---------			
;000,3,RPM									16-18					680-720
;000,4,ECM voltage							170-213				12.0-14.5V						
;000,5,Throttle Valve Angle						0-13					0-5%
;000,6,Idle Regulation							103-180				-5.0-10.0%
;000,7,Idle Stabilization Learned					103-153				-4.9-4.9%
;000,8,O2s b1								116-140				-10.0-10.0%
;000,9,O2s Additive Learned Idle					112-144				-3.0-3.0%
;000,10,O2s Multiplicative Learned Partial Load			116-140				-10.0-10.0
;
;
;
;
001,0,Idling Test						(Bentley 24-109)
001,1,RPM,680-720
001,2,Coolant Temp,85-105
001,3,O2s Before Cat,must fluct +/-2%
001,4,1x111111,adjust. conditions
;
;
002,0,Load Registration					(Bentley 23-46)
002,1,RPM,680-720
002,2,Engine Load
002,3,Injector Period
002,4,Air Mass,1.0-25.0 g/s
;
;
004,0,Gen Engine Data					(Bentley 24-154)
004,1,RPM
004,2,ECM Volts
004,3,Coolant Temp
004,4,Intake Air Temp
;
;
005,0,Engine Operating Mode				(Bentley 24-149)
005,1,RPM
005,2,Engine Load
005,3,Speed,KM/H
005,4,Operating Mode
;
;
014,0,Missfire Recog.					(Bentley 28-27)
014,1,RPM
014,2,Engine Load
014,3,TWC Damaging Msfrs
014,4,Recogn. Status
;
;
015,0,TWC Damaging Missfires				(Bentley 28-29)
015,1,Cyl.1
015,2,Cyl.2
015,3,Cyl.3
015,4,Recogn. Status
;
;
016,0,TWC Damaging Missfires				(Bentley 28-31)
016,1,Cyl.4
016,2,Cyl.5
016,3,Cyl.6
016,4,Recogn. Status
;
;
028,0,Knock Control					(Bentley 28-21)
028,1,RPM,>2000
028,2,Engine Load,>40%
028,3,Coolant Temp,85-105Deg.C
028,4,Test/Results
;
;
030,0,O2s Regulation					(Bentley 24-122)
030,1,O2s Before TWC,xxx
;                      1	control active 
;			    1		operationally ready								
;                    1		heating on
030,2,O2s After TWC,xxx					(Bentley 24-135)
;			    1		control active	
;                    1 		operationally ready
;                   1		heating on
;
032,0,O2s Before TWC Learned Values			(Bentley 24-124)
032,1,O2s Additive
032,2,O2s Multiplicative
;
;
033,0,O2s Before TWC Control						(Bentley 24-126)
033,1,-10.0-10.0,must fluctuate 2%
;
034,0,diag aging of O2s 				(Bentley 26-9)
034,1,RPM
034,2,TWC Temp
034,3,sens dynamics,B1S1
034,4,Status
;
;
036,0,O2s After TWC Operational Readiness		(Bentley 24-137)
036,1,O2s Voltage
036,2,TWC Temp
036,3,Actual Lambda
036,4,Test/results
;
;
041,0,O2s heater Before/After TWC			(Bentley 24-32)
041,2,Before TWC
041,3,O2s After Resistance,Ohm
041,4,After TWC
;
;
046,0,Diag Cat. Converter				(Bentley 26-11)
046,1,RPM
046,2,ConverterTemp,400-650 Deg
046,3,Ampl. Ratio,0.50 Max
046,4,Status
;
;
050,0,A/C Signals						(Bentley 24-177)
050,1,RPM Actual
050,2,RPM Specified
050,3,A/C Status
050,4,Compressor Status
;
;
051,0,Driving Range					(Bentley 24-192)
051,1,RPM
051,2,RPM
051,3,Selector Position
051,4,ECM Voltage
;
;
062,0,Elec. Spd Cntrl					(Bentley 20-40)
062,1,Angl.Snsr.1,3-93%
062,2,Angl.Snsr.2,93-3%
062,3,TP Sensor,12-97%
062,4,Accel.PedalPos.,4-49%
;
;
066,0,Clutch/Brake/Cruise Switches			(Bentley 24-182)
066,2,x1xx Clutch,xx11 Brake				(Bentley 24-187)
066,4,Cruise Buttons,xxxx
;                    0000	switch off 
;                    0001	switch not off
;                    0011	switch on
;			   1011	switch at res
;			   0111	b on A pressed
;
070,0,Evap. System					(Bentley 20-52,01-102)
070,1,Char.Canist.Valve
070,2,Lambda Cntrl.Valve
070,3,Soln.Valve 1
070,4,Test/Result
;
;
071,0,Evap.Emis.Test					(Bentley 20-58,01-100)
071,1,Reed-contact,status
071,2,Error
071,3,Syst.Status
071,4,Test/Result
;
;
;




 


