;
; VAG-COM label file
;
; VW Phaeton (3D)
;
; component: Parking Aid -J446- (#76)
;
; p/n: 3D0 919 283 A
;      3D0 919 283 B
;      3D0 919 283 C
;
; includes measuring blocks and adaptation
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modified: 11/05/2004
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; Measuaring block informations
;
;---------------------------------------------------
;
;
001,0,Direct echo from sensors
001,1,Sensor 1 front,left outside,Specified value: 20...60 cm (255 = invalid/unlimited)
001,2,Sensor 2 front,left center,Specified value: 20...120 cm (255 = invalid/unlimited)
001,3,Sensor 3 front,left inside,Specified value: 20...150 cm (255 = invalid/unlimited)
;
002,0,Direct echo from sensors
002,1,Sensor 4 front,right inside,Specified value: 20...150 cm (255 = invalid/unlimited)
002,2,Sensor 5 front,right center,Specified value: 20...120 cm (255 = invalid/unlimited)
002,3,Sensor 6 front,right outisde,Specified value: 20...60 cm (255 = invalid/unlimited)
;
003,0,Cross echo from sensors
003,1,#1/2 front left,outside/center,Specified value: 20...70 cm (255 = invalid/unlimited)
003,2,#2/3 front left,center/inside,Specified value: 20...150 cm (255 = invalid/unlimited)
003,3,#3/4 front left,inside/right ins.,Specified value: 20...150 cm (255 = invalid/unlimited)
;
004,0,Cross echo from sensors
004,1,#4/5 front right,inside/center,Specified value: 20...150 cm (255 = invalid/unlimited)
004,2,#5/6 front right,center/outside,Specified value: 20...70 cm (255 = invalid/unlimited)
;
005,0,Distance value from sensor
005,1,#1/2 front left,outisde/center,Specified value: 20...70 cm (255 = invalid/unlimited)
005,2,#2/3 front left,center/inside,Specified value: 20...150 cm (255 = invalid/unlimited)
005,3,#3/4 front left,inside/right ins.,Specified value: 20...150 cm (255 = invalid/unlimited)
;
006,0,Distance value from sensor
006,1,#4/5 front right,inside/center,Specified value: 20...150 cm (255 = invalid/unlimited)
006,2,#5/6 front right,center/outside,Specified value: 20...70 cm (255 = invalid/unlimited)
;
007,0,Direct echo from sensor
007,1,#7 rear right,outside,Specified value: 20...60 cm (255 = invalid/unlimited)
007,2,#8 rear right,center,Specified value: 20...120 cm (255 = invalid/unlimited)
007,3,#9 rear right,inside,Specified value: 20...150 cm (255 = invalid/unlimited)
;
008,0,Direct echo from sensor
008,1,#10 rear left,inside,Specified value: 20...150 cm (255 = invalid/unlimited)
008,2,#11 rear left,center,Specified value: 20...120 cm (255 = invalid/unlimited)
008,3,#12 rear left,outside,Specified value: 20...60 cm (255 = invalid/unlimited)
;
009,0,Cross echo from sensor
009,1,#7/8 rear right,outisde/center,Specified value: 20...70 cm (255 = invalid/unlimited)
009,2,#8/9 rear right,center/inside,Specified value: 20...150 cm (255 = invalid/unlimited)
009,3,#9/10 rear right,inside/left ins.,Specified value: 20...150 cm (255 = invalid/unlimited)
;
010,0,Cross echo from sensor
010,1,#10/11 rear left,inside/center,Specified value: 20...150 cm (255 = invalid/unlimited)
010,2,#11/12 rear left,center/outside,Specified value: 20...70 cm (255 = invalid/unlimited)
;
011,0,Distance value from sensor
011,1,#7/8 rear right,outisde/center,Specified value: 20...70 cm (255 = invalid/unlimited)
011,2,#8/9 rear right,center/inside,Specified value: 20...150 cm (255 = invalid/unlimited)
011,3,#9/10 rear right,inside/left ins.,Specified value: 20...150 cm (255 = invalid/unlimited)
;
012,0,Distance value from sensor
012,1,#10/11 rear left,inside/center,Specified value: 20...150 cm (255 = invalid/unlimited)
012,2,#11/12 rear left,center/outside,Specified value: 20...70 cm (255 = invalid/unlimited)
;
013,0,Total distance
013,1,Left front,total distance,Specified value: 20...150 cm (255 = invalid)
013,2,Right front,total distance,Specified value: 20...150 cm (255 = invalid)
013,3,Right rear,total distance,Specified value: 20...150 cm (255 = invalid)
013,4,Left rear,total distance,Specified value: 20...150 cm (255 = invalid)
;
014,0,Voltages
014,1,Supply voltage,,Specified value: 8.7...16.7 V
014,3,Sensor,supply voltage,Specified value: 7.2...9.2 V
014,4,Display-/speaker,supply voltage,Specified value: 7.5...16.5 V
;
015,3,Button,status,Specified value: 0 = not pressed/1 = pressed
;
016,1,Automatic,transmission,Specified value: 0 = not installed/1 = installed
016,2,Selector,lever position,Specified values: 00/01/02/03/12/14
016,3,Parking,brake,Specified value: 0 = inactive/1 = active
;
017,1,Trailer,,Specified value: 0 = not mounted/1 = mounted
017,2,Trailer,control module,Specified value: 0 = not installed/1 = installed
017,3,Vehicle Speed,Specified value: 0...250 km/h
017,4,Speed shut-off,,Specified value: 0 = inactive/1= active
;
018,1,Terminal 15,status,0 = off/1 = on
018,2,System status,,0 = inactiv/1 = activ
018,3,Display,brightness,Specified value: 50...100 %
018,4,Acoustic,warning,0 = inactiv/1 = activ
;
;
;---------------------------------------------------
;
; Adaptation informations
;
;---------------------------------------------------
;
;
A01,0,Front Buzzer Volume
A01,5,Front Buzzer Volume
A01,6,Adaptation of the warning buzzer volume.
A01,7, 
A01,8,Range: 0 - 100 %
;
A02,0,Rear Buzzer Volume
A02,5,Rear Buzzer Volume
A02,6,Adaptation of the warning buzzer volume.
A02,7, 
A02,8,Range: 0 - 100 %
;
A03,0,Shut-off speed
A03,5,Shut-off speed
A03,6,Adaptation of the parking aid shut-off speed.
A03,7, 
A03,8,Range: 1 - 15
A03,9,Standard value: 14
;
A04,0,Offset distance
A04,5,Offset distance
A04,6,Here you can enter an additional distance (in cm)
A04,7,to be added to rear measurements to allow for
A04,8,the presence of a trailer hitch.
A04,9, 
A04,10,Range: 1 - 30 cm
;
