;A. Ferron Email:iso9141@yahoo.ca
;Controller number 1C0-959-799-C
;Generation 3 Beetle and Jetta
;
;
1,0,Display Group - 1 -:(Driver's side door)See Note
1,1,L.F.Switch-E40-,auto.open/closed,man.open/closed,not oper,implausible
1,2,L.F.Thermal protection,(Yes/No)
1,3,Safety switch,Rear-E39-,off/on,not installed
1,4,Blank
;
;
2,0,Display group -2 -:(Driver's side door Arm rest)See Note
2,1,R.F.Switch-E81-,auto.open/closed,man.open/closed,not oper.implausible
2,2,L.R.Switch-E53-,auto.open/closed,man.open/closed,not oper.implausible
2.3.R.R.Switch-E55-,auto.open/closed,man.open/closed,not oper.implausible
2,4,Blank
;
;
3,0,Display group -3 -:(Driver's side door Mirror Switch)See Note
3,1,Mirror Sw.-E43-,Pos X+/X-,Y+/Y-,not operated,implausible,not installed
3,2,Mirror Sel.Sw.-E48-,left/right,fold out,not operated,implausible,not installed,A K 1J
3,3,Mirror Folding Sw.-E263-,disengaged/engaged,not installed,empty,A K 2J
3,4,Mirror heating-E231-,on/off,not installed, A K 3J
;K Notes:
;1J On right-hand drive vehicles, this dimension value is inverted. Selecting the left 
;window, the right is displayed and instead of the right, the left.
;2J Measured value is displayed only when the switch is installed.
;3J Ignition must be switched on.
;
;
4,0,Display Group -4 -: (Passenger's side Door)
4,1,R.F.Switch-E107-,auto.open/closed,man.open/closed,not operated,implausible,not installed
4,2,R.F.Thermo protection,Yes/No,not installed
4,3,Mirror Folding Sw.-E263-,disengaged/engaged,not installed),A K 2J
4,4,Blank
;K Notes:
;Measured value is displayed for right-hand drive vehicles only if the switch is installed.
;
;
5,0,Display group -5 -: (Rear Doors) 
5,1,L.R.Window Sw-E52-,auto.open/closed,man.open/closed,not operated,implausible,not installed
5,2,L.R.Thermo protection,Yes/No,not installed
5,3,R.R.Window Sw-E54-,auto.open/closed,man.open/closed,not operated,implausible,not installed
5,4,R.R.Thermo protection,Yes/No,not installed
;
;
6,0,Display Group -6 -: (Central Control Module)
6,1,Voltage Supply,Terminal 30,Voltage [V]
6,2,Ign.terminal 15,Terminal 15 on,terminal15 off,no communication
6,3,S-contact,operated/not operated,no communication
6,4,Vehicle Speed,Speed in Km/h
;
;
7,0,Display Group -7 -: (Front Doors)
7,1,Key Switch L.F.,open/closed,not operated,implausible
7,2,Key Switch,R.F.,open/closed,not operated,implausible
7,3,L.F.Interior,lock Sw.-E150-,locking/unlocking,not operated,implausible
7,4,R.F.Interior Lock Sw.-E198-,locking/unlocking,not operated,implausible,empty
;
;
8,0,Display Group -8 -: (Central Control Module)
8,1,Hood Alarm,Switch-F120-,open/closed,not installed,no communication
8,2,Trunk Lid Release, Switch-E165-,open/closed,not operated,implausible
8,3,Trunk Lock/Alarm/Central,Locking Switch-F124-,open/closed,no communication)
8,4,Thermal protection,for central locking,(yes/no)
;
;
9,0,Display Group -9 -: (Central Control Module)
9,1,L.F.door locking,locked/unlocked,safe,not installed,implausible
9,2,R.F.door locking,locked/unlocked,safe,not installed,implausible
9,3,L.R.door locking,locked/unlocked,safe,not installed,implausible
9,4,R.R.door locking,locked/unlocked,safe,not installed,implausible)
;
;
10,0,Display Group -10 -: (Front/Rear Doors)
10,1,L.F.rotory switch,Door open,Door closed
10,2,R.F.rotory switch,Door open,Door closed
10,3,L.R.rotory switch,Door open,Door closed,not installed A K
10,4,R.R.rotory switch,Door open,Door closed,not installed,empty
;K Notes:
;In some models, there is common rotor switch wiring for both rear doors.
;
;
11,0,Display Group -11 -: (Central Control Module)
11,1,Key recog.immo.,yes/no,not installed,no communication)
11,2,Auto.central locking sw.,not oper/operated,not installed
11,3,Unlocking sunroof,wind screen,on/off,yes/no
11,4,CAN-Bus Condition,Single wire,dual wire
;
;
12,0,Display Group -12 -: (Central Control Module)
12,1,L.F.CAN-Bus Condition,L.F.door 0,L.F.door 1,empty
12,2,R.F.CAN-Bus Condition,R.F.door 0,R.F.door 1,empty
12,3,L.R.CAN-Bus condition,L.R.door 0,L.R.door 1,empty
12,4,R.R.CAN-Bus condition,R.R.door 0,R.R.door 1,empty
;
;
13,0,Display Group -13 -: (Central Control Module)See notes
13,1,Trunk remote-E188-,and rear switch-E234-,not operated,remote switch,lid lever,implausible
13,2,Trunk pre-latch,open/closed,not installed
13,3,Inst.panel light,0 to 100%,not installed,A K
; in 16 stages
3,4,Comfort window reg.sw.,auto.open/closed,man.open/closed,not oper,implausible,not installed
;K Note:Head lamp Sw.light must be ON
;
;
14,0,Display Group -14 -: (Central Control Module)
14,1,Fixed code known,OK/not OK,no measured value
14,2,Code in signal range,OK/not OK,no measured value
14,2,Algorithm,OK/not OK,no measured value
14,3,Key number,(1/2/3/4),0=not operated
;
;
15,0,Display Group -15 -: (Central Control Module)
15,1,Remote control buttons,open/closed,trunk/panic,0 or 1
15,2,Interior Monitoring-G273-,yes/no,not installed
15,3,Interior Monitoring,Deactivation Switch-E267-,yes/no,not installed
;
;
16,0,Display Group -16 -: (Central Control Module)See note
16,1,Last alarm,0 to 65535
16,2,2nd Last alarm,0 to 65535
16,3,3rd Last alarm,0 to 65535
16,4,4th Last alarm,0 to 65535
;
;
;Possible values:
;1   = Driver's side door terminal 
;2   = Passenger's side door terminal 
;4   = Rear left door terminal
;8   = Rear right door terminal
;16  = Luggage compartment flap
;17  = Anti-theft immobilizer recognition
;18  = Speaker backup
;32  = Hood contact
;64  = Ignition terminal 15
;128 = Interior monitoring
;255 = No alarm operation
