;
; VAG-COM label file
;
; Audi A3 (8P) / Audi TT (8N) / Seat Altea (5P) / Seat Toledo (5P)
; Skoda Octavia (1Z) / VW Golf (1K) / VW New Beetle (1C) / VW Touran (1T)
;
; component: Transmission Electronic (#02) - 6-Speed Automatic Transmission 09G
;
; p/n: 09G 927 750 ???
;
; includes measuring blocks
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 17/05/2004
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; Measuring block informations
;
;---------------------------------------------------
;
;
001,1,Engine speed,,Specification: 0...7650 RPM
001,2,Transmission,RPM (from G182),Specification: 0...7650 RPM
001,3,Transmission,Output RPM,from G195 (Specification: 0...7650 RPM)
001,4,Driving Mode,,see Labelfile
;  0 = Neutral
;  R = Reverse gear
;  N = Neutral
; 1H = 1. Gear hydraulic
; 1M = 1. Gear mechanic
; 2H = 2. Gear hydraulic
; 2M = 2. Gear mechanic
; 3H = 3. Gear hydraulic
; 3M = 3. Gear mechanic
; 4H = 4. Gear hydraulic
; 4M = 4. Gear mechanic
; 5H = 5. Gear hydraulic
; 5M = 5. Gear mechanic
; 6H = 6. Gear hydraulic
; 6M = 6. Gear mechanic
;
002,1,Transmission RPM,(from G182),Specification: 0...1650 RPM
002,2,G182 Voltage,Transmission RPM,Specification: 0...5.00 V
002,3,Transmission,output RPM,from G195 (Specification: 0...7650 RPM)
002,4,G195 Voltage,Transmission RPM,Output (Specififcation: 0...5.00 V)
;
003,1,Driving Manner,,Specification: DS/SO/WU/TT/AS/AC
003,2,Accelerator pedal,position,Specification: 0...100 % / Kick-Down / Error
003,3,Vehicle Speed,,Specification: 0...255 km/h
003,4,Driving Mode,,see Labelfile
;  0 = Neutral
;  R = Reverse gear
;  N = Neutral
; 1H = 1. Gear hydraulic
; 1M = 1. Gear mechanic
; 2H = 2. Gear hydraulic
; 2M = 2. Gear mechanic
; 3H = 3. Gear hydraulic
; 3M = 3. Gear mechanic
; 4H = 4. Gear hydraulic
; 4M = 4. Gear mechanic
; 5H = 5. Gear hydraulic
; 5M = 5. Gear mechanic
; 6H = 6. Gear hydraulic
; 6M = 6. Gear mechanic
;
004,1,Selector Lever,Position,Specification: P/R/N/D/S/Manual/Error
004,2,Accelerator pedal,position,Specification: 0...100 % / Kick-Down / Error
004,3,Declination,Recognition,Specification: UP = upward / LEVEL = no declination / DW = downward
004,4,Driving Mode,,see Labelfile
;  0 = Neutral
;  R = Reverse gear
;  N = Neutral
; 1H = 1. Gear hydraulic
; 1M = 1. Gear mechanic
; 2H = 2. Gear hydraulic
; 2M = 2. Gear mechanic
; 3H = 3. Gear hydraulic
; 3M = 3. Gear mechanic
; 4H = 4. Gear hydraulic
; 4M = 4. Gear mechanic
; 5H = 5. Gear hydraulic
; 5M = 5. Gear mechanic
; 6H = 6. Gear hydraulic
; 6M = 6. Gear mechanic
;
005,1,Hill Driving,Factor,Specification: -32...+31.6
005,2,Throttle valve,factor,Specification: 0...100 %
005,3,Dynamic Index,,Specification: 0...100 %
005,4,Accelerator pedal,position,Specification: 0...100 % / Kick-Down / Error
;
006,1,ATF Temperature,(G93),Specification: -50...+171 °C
006,2,Specified Current,Solenoid Valve 4,N91 (Specification: 0...1.000)
006,3,Lock-Up Clutch,Slip Condition,Specification: 0 = open / 1 = closed / 2 = slipped
006,4,Lock-Up Clutch,Slip Condition,Specification: -1250...+1250 RPM
;
007,1,Solenoid Valve 5,(N92),Specification: 0...1.000 A
007,2,Solenoid Valve 9,(N282),Specification: 0...1.000 A
007,3,Solenoid Valve 3,(N90),Specification: 0...1.000 A
007,4,Solenoid Valve 10,(N283),Specification: 0...1.000 A
;
008,1,Solenoid Valve 6,(N93),Specification: 0...1.000 A
008,2,Solenoid Valve 4,(N91),Specification: 0...1.000 A
008,3,Solenoid Valve 1,Solenoid Valve 2,N88/N89 (Specification: 0 = inactive / 1 = active)
008,4,Battery,Voltage,Specification: 0...25.5 V
;
009,1,Brake Pedal,Switch,Specification: 0 = not operated / 1 = operated
009,2,Kick-Down,Switch,Specification:  = not operated / 1 = operated
009,3,Selector Lever,Position,Specification: P/R/N/D/S/Manual/Error
009,4,Multi-Function,Switch
;
010,1,ATF Temperature,,Specification: -50...+171 °C
010,2,ATF Temperature,Sensor Voltage
010,3,Transmission,Condition
010,4,Voltage Supply,,Specification: 0...25.5 V
;
011,1,Brake Pedal Switch,Condition (F47),Specification: ON = switch operated / OFF = switch not operated
011,2,Locking in P/N,Condition
011,3,Speed,,Specififcation: 0...255 km/h
011,4,Selector Lever,Position,Specification: P/R/N/D/S/Manual/Error
;
012,1,Selector Lever,Position,Specification: P/R/N/D/S/Manual/Error
012,2,Tiptronic,Recognition
012,3,Driving Mode,,see Labelfile
;  0 = Neutral
;  R = Reverse gear
;  N = Neutral
; 1H = 1. Gear hydraulic
; 1M = 1. Gear mechanic
; 2H = 2. Gear hydraulic
; 2M = 2. Gear mechanic
; 3H = 3. Gear hydraulic
; 3M = 3. Gear mechanic
; 4H = 4. Gear hydraulic
; 4M = 4. Gear mechanic
; 5H = 5. Gear hydraulic
; 5M = 5. Gear mechanic
; 6H = 6. Gear hydraulic
; 6M = 6. Gear mechanic
012,4,Transferrable,Torque,Specification: 0...100
;
013,1,Selector Lever,Position,Specification: P/R/N/D/S/Manual/Error
013,2,Multi-Function,Switch Position
013,3,Tiptronic,Recognition
013,4,Transferrable,Torque,Specification: 0...100
;
014,1,Accelerator pedal,position,Specification: 0...100 %
014,2,[N/A]
014,3,Idle Switch,Condition,Specification: 0 = not operated / 1 = operated
014,4,Accelerator Pedal,Condition,Specification: 0 = not depressed / 1 = depressed
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine
125,2,Brake Electronics
125,3,Instrument Cluster
125,4,All-Wheel-Drive
;
