;
; VAG-COM Measuring Block Labels for
; VW COMFORT CONVENIENCE 1C0-959-799-C
; 
; contributed by:
;
; MOGolf @ WWW.TDICLUB.COM
;
; Information from Bentley repair CD
; for Golf and Jetta
; this applies to modules from 06.01 on
; until they start using something else
;
1,0,Driver's door (DD) switches 
1,1,Hall signal
; auto. open
; auto. close
; man. open
; man. close
; close not operated
; implausible
1,2,Thermal protect.
; yes
; no
1,3,Child safety sw.
; off
; on
; not installed
1,4,Empty
;
2,0,Driver's Door (DD) Switches 
2,1,Pass. Window,Switch
2,2,LR Window,Switch
2,3,RR Window,Switch
2,4,Empty
;
3,0,Driver's door switches
3,1,Mirror adjust.
3,2,Mirror select.
3,3,Empty
3,4,Mirror heating
;
4,0,Passenger Door switches
4,1,Window Switch
4,2,Thermal protect.
4,3,Empty
4,4,Empty
;
5,0,Rear doors
5,1,LR window,switch
5,2,LR thermal,protection
5,3,RR window,switch
5,4,RR thermal,protection
;
6,0,Signals
6,1,Vehicle,voltage
6,2,Ignition
6,3,S-contact
6,4,Speed 
;
7,0,Dr. and P. Doors
7,1,Dr. key,switch
7,2,P. key,switch
7,3,Dr. interior,lock switch
7,4,P. interior,lock switch
;
8,0,Central control unit
8,1,Hood contact,switch
8,2,Rear lid/tail.,key
8,3,Rear lid/tail.,contact
8,4,Thermo. protect.
;
9,0,Central control unit
9,1,Driver's,feedback
9,2,Pass.,feedback
9,3,Left rear,feedback
9,4,Right rear,feedback
;
10,0,Central control unit
10,1,Dr. latch,switch
10,2,P. latch,switch
10,3,LR. latch,switch
10,4,RR. latch,switch
;
11,0,Central control unit
11,1,Immo. key,recognition
11,2,Auto lock/unlock
11,3,Sunroof,released
11,4,Data bus,Two-wire
;
12,0,Door control units
12,1,Driver side, 1=OK
12,2,Pass. side, 1=OK
12,3,Right rear, 1=OK
12,4,Left Rear, 1=OK
;
13,0,Central control unit
13,1,Rear lid,button/handle
13,2,Rear first,detent
13,3,Instrument,Illumination
13,4,Empty
;
14,0,Central Control unit
14,1,Perm. code,known
14,2,Code within,effect. range
14,3,Algorithm
14,4,Key number
;
15,0,Central Control unit
15,1,RC key button,l/ul/rlr/panic
15,2,Int. monitor,sensor
15,3,Int. monitor,swtich-off
15,4,Empty
;
16,0,Alarm sources
16,1,Last,see label file
16,2,2nd last,see label file
16,3,3rd last,see label file
16,4,4th last,see label file
;1=rear lid/tailgate contact switch
;2=right rear rotary latch switch
;4=left rear rotary latch switch
;8=fr. pass. rotary latch switch
;16=ignition
;17=immobilizer
;32=interior monitoring
;64=hood contact switch
;128=dr. rotary latch switch
;255=no alarm