;
; VAG-COM Measuring Block Labels file.
; Module 17 -- Instrument Cluster
; 
; from USA 2001 Audi A6 2.7T 6sp
;
; ECU p/n :     4B0-920-981-G
; Component:    C5-KOMBIINSTR. VDO D12
; Soft coding:  02264
;
; Modification history
; created:  Richard Solomon,  22 May 2002
;
;
;
;
1,0,Main Gauges
1,1,Road Speed
1,2,Engine Speed,(RPM)
1,3,Oil Pressure,OK | Min
1,4,Clock Time
;
2,0,Main Gauges
2,1,Odometer,(/10)
2,2,Fuel Gauge,(Liters)
2,3,Fuel Sensor,Resistance
2,4,Outside Air,Temperature
;
3,0,Coolant Temperature
3,1,Coolant,Temperature
3,2,
3,3,
3,4,
;
4,0,Undocumented
4,1,
4,2,
4,3,
4,4,
;
10,0,Adaptation Channels and Values
10,1,Fuel Sender,Channel
10,2,Fuel Sender,Adjustment
10,3,Odometer,Channel
10,4,Odometer,(/10)
;
11,0,Adaptation Channels and Values
11,1,DIS Language,Channel
11,2,DIS Language,1=Ger. 2=Eng.
11,3,Miles To Empty,Adj. Channel
11,4,Miles To Empty,Adj. %
;
12,0,Service Indicator Adaptation Channels and Values
12,1,Dist. since Service,Channel
12,2,Dist. since Service,(/100?)
12,3,Days since Service,Channel
12,4,Days since Service
;
13,0,Service Indicator Adaptation Channels and Values
13,1,Minimum Miles,Channel
13,2,Minimum Miles,(/1000)
13,3,Maximum Miles,Channel
13,4,Maximum Miles,(/1000)
;
14,0,Service Indicator Adaptation Channels and Values
14,1,Maximum Time,Channel
14,2,Maximum Time,Days
14,3,
14,4,
;
15,0,Adaptation Channels and Values
;
16,0,Adaptation Channels and Values
;
22,0,Immobilizer III: Status
22,1,Start permitted
22,2,ECM Responding,(Engine Started)
22,3,Key Ok
22,4,Number of keys
;
23,0,Immobilizer III: Key Status
23,1,Variable code Ok
23,2,Key Status
23,3,Fixed code Ok
23,4,Immobilizer Status
;
24,0,Immobilizer III: Lockout Times (minutes)
24,1,Cluster Login
24,2,ECM Login
24,3,
24,4,Transponder (key),Recognition
;
25,0,Immobilizer III: CAN Status
25,1,ECM Communications
25,2,,
25,3,,
25,4,,
;
50,0,Main Gauges
50,1,Odometer,(/10)
50,2,Engine Speed,(RPM)
50,3,Oil,Temperature
50,4,Coolant,Temperature
;
80,0,?Cluster Mfg String?
80,1,
;
81,0,VIN / Immobilizer ID
81,1,
;
125,0,CAN Communications
;
126,0,CAN Communications
;
130,0,CAN Communications
;
140,0,CAN Communications
;
; End of File