;
; VAG-COM Measuring Block Labels 
; Engine Code AFX;AFV;AFW
; Motronic MP 9.0
; 1HS 908 258 x
; source: workshop manual          
: Golf 1992,Vento 1992
: Edition 04.96
;
;0,0,See label file
;0,1,Intake Air Temp
;0,2,Batt Voltage
;0,3,Coolant Temp
;0,4,Engine load
;0,5,O2 Sensor
;0,6,O2 Sensor; learned value
;0,7,Operating Cond
;0,8,Throttle Angle
;0,9,Injection Time
;0,10,Engine Speed
;
1,0, General Engine Data
1,1,RPM
1,2,coolant temp
1,3,lambda volts
1,4,adjustment cond.,see LBL file
;                           xxxxxxxx
;                           1 Fault in fault memory
;                            1 Signal from automatic transmission
;                             1 Air conditioner on
;                              1 Idle switch open
;                               1 not relevent
;                                1 not relevent
;                                 1 Idle speed too high
;                                  1 Coolent temp below 80'C
2,0,Injection Control
2,1,RPM 
2,2,Injection  period
2,3,Battery volts
2,4,Intake Air Temp
;
3,0,Control Input
3,1,RPM
3,2,Engine load
3,3,Throttle angle
3,4,Throttle volts
;
4,0,Dynamic Data
4,1,RPM
4,2,Engine Load
4,3,Speed
4,4,operating cond.,see LBL file 
;                            xxxxxxxx
;                            1 Overrun
;                             1 Idling
;                              1 Part load
;                               1 Full load
;                                1 Acceleration enrichment
;                                 1 Not relevant
;                                  1 Air conditioner signal
;                                   1 Cylinder #1 recognised
10,0,Ignition, Knock sensor adjustments
10,1,timing cyl#1
10,2,timing cyl#2
10,3,timing cyl#3
10,4,timing cyl#4
;
;eor