;
; VAG-COM Measuring Block Labels for
; VW COMFORT CONVENIENCE 1J0-959-799-aj
; 
; contributed by:
;
; Eric Klobas
; University Volkswagen Audi
; Seattle, WA, USA
;
; additions by Mike Sauve www.alientech.net
; changed RF/LF to Driver's Door/Pass door to support RHD cars
; added "Protection" labels, added alarm source codes
;
1,0,Driver's door (DD) switches mjs
1,1,RearWinLock
1,2,DD lock switch
1,3,DD Window Motor
1,4,
;
2,0,Driver's Door (DD) Switches 
2,1,DD WindowSw
2,2,Pass Window Switch
2,3,LR Window Switch
2,4,RR Window Switch
;
3,0,Driver's door switches
3,1,DD key switch 
3,2,DD Latch/Protection
;protection is thermal protector, shuts off pwr
; window for 10 seconds on overload
3,3,DD latch feedback
3,4,DD C/L feedback
;
4,0,Mirrors
4,1,DD Mirror Sw U/D
4,2,DD mirror Sw L/R
4,3,DD folding mirror
4,4,Empty
;
5,0,Passenger door switches
5,1,Pass window switch
5,2,Pass Lock switch
5,3,Pass folding mirror
;
6,0,Passenger door
6,1,Pass key switch
6,2,Pass latch/protect
6,3,Pass latch fdback
6,4,Pass C/L feedback
;
7,0,RR door
7,1,RR window sw
7,2,RR latch/protect
7,3,RR latch fdback
7,4,RR C/L feedback
;
8,0,LR door
8,1,LR window sw
8,2,LR latch/protect
8,3,LR latch fdback
8,4,LR C/L feedback
;
9,0,signals
9,1,inst light sig
9,2,Car Speed (G22)
9,3,Key remote sig
9,4,Interior Mon
;
10,0,Sgnals
10,1,S contact
10,2,Mirror heat
10,3,Trunk lock 
10,4,T15 on/off
;
11,0,Signals
11,1,hood&Radio sw
11,2,trunk latch sw
11,3,Sunroof Sync
11,4,C/L temp sw
;
12,0,
12,1,CAN Bus
12,2,opt fr equip
12,3,opt rr equip
12,4, opt equip
;
13,0,remotes
13,1,Permanent code
13,2,Code in range
13,3,Algorithm
13,4,Key number,(press remote)
;
14,0,Central Convenience module
14,1,Terminal 30
14,2,Rear unlatch sig
14,3,Interior Mon
14,4,Thermo protect,DS/PS/RL/RR
;
15,0,Alarm sources
15,1,Last,(see label file)
15,2,2nd,(see label file)
15,3,3rd,(see label file)
15,4,4th,(see label file)
;
;1 = rear lid
;2 = RR door
;4 = LR door
;8 = Pass door
;16= Ignition
;32= Interior monitor
;64= Hood
;128=Driver's door
;255=no alarm
;
16,0,Auto locks
16,1,Imob key recogn
16,2,auto int lock Sw
16,3,Rear latch detent
16,4,
;