;
; VAG-COM label file
;
; VW Phaeton (3D)
;
; Component: Steering Wheel Electronics -J453- (#16)
;
; p/n: 3D0 953 549 B
;      3D0 953 549 C
;      3D0 953 549 D
;      3D0 953 549 E
;
; includes measuring blocks
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modified: 11/05/2004
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; Measuaring block informations
;
;---------------------------------------------------
;
;
001,1,Blinker,,Specified value: not active/left/right
001,2,Headlamp,flasher,Specified value: not active/active
001,3,High beam,,Specified value: not active/active
001,4,Signal horn,,Specified value: not active/active
;
002,1,Wiping,,Specified value: not active/Interval/Level 1/Level 2
002,2,Interval,potentiometer,Specified value: off/Interval 1/2/3/Poti Ok
002,3,Front washing,,Specified value: not active/active
002,4,Voltage,terminal 30
;
003,1,Steering column,adjustment,Specified value: not active/raise/lower/forward/backward
003,2,Easy Entry,switch,Specified value: on/off
;
004,0,CSO-Signal
004,1,Terminal P,,Specified value: on/off
004,2,Terminal S,,Specified value: on/off
004,3,Terminal X,,Specified value: on/off
004,4,Terminal 15,,Specified value: on/off
;
005,1,Terminal X,switched on,,Specified value: yes/no
005,2,Heatet seat,status,Specified value: off/Level
005,3,St. wheel heater,via VSCM,Specified value: yes/no
005,4,St. wheel heater,via control head,Specified value: yes/no
;
006,0,Steering Wheel Heating
006,1,Status,heater,Specified value: not installed/on/off
006,2,Temperature,sensor,Specified value: not installed/Temp. value
;
007,1,Dimming,value,steering wheel illumination
;
011,0,Cruise Control System (CCS)
011,1,CCS+ switch,,Specified value: not active/active
011,2,CCS- switch,,Specified value: not active/active
011,3,SET button,,Specified value: not active/active
011,4,RESET,button,Specified value: not active/active
;
012,1,CANCEL,button,Specified value: not active/active
012,2,CCS ON/OFF,button,Specified value: not active/active
012,3,Illumination,button,Specified value: not active/active
;
013,1,Vol+ button,,Specified value: not active/active
013,2,Vol- button,,Specified value: not active/active
013,3,Telephone,button,Specified value: not active/active
013,4,PTT button,,Specified value: not active/active
;
014,1,Button OK,,Specified value: not active/active
014,2,Abort button,,Specified value: not active/active
014,3,Menu button,,Specified value: not active/active
;
015,1,Scroll-knurling,wheel
015,3,ADR knurling,wheel
;
