;
; VAG-COM label file
;
; VW Phaeton (3D)
;
; component: Distance Regulation -J428- (#13)
;
; p/n: 3D0 907 563 B
;      3D0 907 563 C
;
; includes measuring blocks
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modified: 11/05/2004
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; Measuaring block informations
;
;---------------------------------------------------
;
;
001,0,Wheel speed
001,1,Left front,wheel speed,Specified value: 0...255 km/h
001,2,Right front,wheel speed,Specified value: 0...255 km/h
001,3,Left rear,wheel speed,Specified value: 0...255 km/h
001,4,Right rear,wheel speed,Specified value: 0...255 km/h
;
002,1,Buttons CCS+/-,SET/RESET,Specified value: active/inactive
002,2,Buttons CANCEL,Wheel/ON/OFF,Specified value: active/inactive
;
003,1,TRM+ supply,,Specified value: 0...5.1 V
003,2,TRM- supply,,Specified value: 0...5.1 V
003,3,Battery voltage,,Specified value: 0...16 V
;
006,1,Horizontal,adjustment,Specified value: -12.7...+12.7 °
006,2,vertical,adjustment,Specified value: -12.7...+12.7°
;
007,1,Operations of,button CCS+,Specified value: -10...+10
007,2,Operating button,for CCS,Specified value: -10...+10
007,3,Laser pointer,quadrant,Specified value: 1...4
;
008,1,ADR status
008,2,CCS status
008,3,SET speed,,Specified value: 0....255 km/h
;
009,1,Sensor,temperature,Specified value: -40...+125 °
;
010,1,Distance,to object,Specified value: 0...180 m
010,2,Angle to,object,Specified value: -6.35...+6.35 °
010,3,Object speed,,Specified value: -255...+255 km/h
;
011,3,Steering wheel,turning angle,Specified value: -720...+720 °
;
012,1,CANCEL button,,Specified value: off/on
012,4,ESP-shut-off,,Specified value: off/on
;
013,1,Brake pedal,,Specified value: off/on
;
